| TIBURON(GK) >2007 > G 2.7 DOHC > Body Electrical System > Lighting System>Repair procedures |

REPLACEMENT OF LAMPS
HEAD LAMP/TURN SIGNAL LAMP
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front bumper upper cover(A).
3. | Loosen the mounting bolts (3EA) of head lamp. Remove the head lamp assembly(A).
Take care that retaining clip is not to be damaged.
4. | Disconnect the head lamp connector(A).
5. | Remove the head lamp bulb after removing the cap turning in counterclockwise direction. A : Low beam head lamp B : High beam head lamp C : Turn signal lamp D : Side marker lamp
6. | Installation is the reverse of removal.
TURN SIGNAL LAMP
1. | Disconnect the negative (-) battery terminal.
2. | Remove the rear woofer speaker panel (A).
3. | Loose the nuts (3EA) holding the rear combination lamp then disconnect the connector then remove the rear combination lamp(A).
4. | Replace the bulbs turning in counterclockwise direction after disconnecting the rear combination lamp assembly. A : Tail / Stop lamp B : Tail / Stop lamp C : Turn signal lamp D : Back up lamp E : Side marker
5. | Installation is the reverse of removal.
FRONT FOG LAMP
1. | Disconnect the negative(-) battery terminal.
2. | Remove the front bumper. (Refer to Body group - "Front bumper")
3. | Remove the front fog lamp assembly (A) after disconnecting the front fog lamp connector and loosening 3 screws.
4. | Installation is the reverse of removal.
CENTER HIGH MOUNTED STOP LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the rear spoiler after removing 4 nuts. (External spoiler type)
3. | Remove the center high mounted stop lamp assembly.
4. | Installation is the reverse of removal.
LICENSE PLATE LAMP
1. | Disconnect the negative battery terminal.
2. | Detach the lamp from front bumper assembly with a flat-tip screwdriver and disconnect the lamp connector.
3. | Installation is the reverse of removal.
OVERHEAD CONSOLE LAMP
1. | Disconnect the negative battery terminal.
2. | Detach the map lamp lens from the lamp assembly with a flat-tip screwdriver.
3. | Detach the lamp assembly from the headliner after removing the 4 screws.
4. | Disconnect the wiring connectors from the headliner.
5. | Installation is the reverse of removal.
LUGGAGE LAMP
1. | Disconnect the negative battery terminal.
2. | Detach the luggage lamp assembly from the luggage side trim with a flat-tip screwdriver.
3. | Installation is the reverse of removal.
INSPECTION OF COMPONENTS
HEAD LAMP RELAY
1. | Remove the head lamp relay from the relay box in the engine compartment.
2. | Check for continuity between terminals on the relay.
HAZARD LAMP SWITCH
1. | Disconnect the negative (-) battery terminal.
2. | Remove the center facia panel (B) after opening the astray(A).
3. | Disconnect the hazard lamp switch conector(A).
4. | Operate the switch and check for continuity between terminal No.3 and No.11 with an ohmmeter.
RHEOSTAT
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the rheostat connector from the crash pad panel.
3. | Check for intensity. If the light intensity of the lamps changes smoothly without any flickering when the rheostat is turned, it can be assumed that the rheostat is normal.
FRONT FOG LAMP SWITCH
1. | Disconnect the negative (-) battery terminal.
2. | Remove the center facia panel (B) with scraper after opening the astray (A).
3. | Disconnect the front fog lamp switch connector (A).
4. | Operate the switch and check for continuity between terminal No.4 and No.16 with an ohmmeter.
MAP LAMP SWITCH