| TIBURON(GK) >2007 > G 2.7 DOHC > Engine Mechanical System > Intake And Exhaust System > Intake Manifold>Repair procedures |

REMOVAL
1. | Remove the engine cover.
2. | Remove air cleaner hose.
3. | Remove surge tank assembly.
(1) | Disconnect the accelerator cable.
(2) | Disconnect the TPS connector.
(3) | Disconnect the ISA connector.
(4) | Disconnect the injector connector.
(5) | Disconnect the PCSV connector.
(6) | Disconnect the PCSV hose.
(7) | Disconnect the brake booster vacuum hose.
(8) | Disconnect the PCV hose.
(9) | Disconnect the IAT sensor connector.
(10) | Remove the surge tank stay.
(11) | Remove the surge tank assembly.
4. | Remove the injector assembly(A).
5. | Remove the intake manifold(A) and gasket.
INSTALLATION
1. | Install the intake manifold and gasket.
Tightening torque 18.6 ~ 23.5Nm (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
2. | Install the injector assembly. (Refer to Injector in FL Group).
3. | Install the surge tank assembly.
(1) | Install the surge tank assembly.
Tightening torque 18.6 ~ 23.5Nm (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
(2) | Install the surge tank stay.
Tightening torque 18.6 ~ 23.5Nm (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
(3) | Install the ground cable.
(4) | Connect the IAT sensor connector.
(5) | Connect the PCV hose.
(6) | Connect the brake booster vacuum hose.
(7) | Connect the PCSV hose.
(8) | Connect the PCSV connector.
(9) | Connect the injector connector.
(10) | Connector the ISA connector.
(11) | Connector the TPS connector.
(12) | Connector the actuator cable.
4. | Install the air cleaner hose.
5. | Install the engine cover.