| TIBURON(GK) >2007 > G 2.7 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM)>Troubleshooting |

DESCRIPTION
HI-SCAN CHECK
1. | Turn the ignition switch off.
2. | Connect the scantool connector to the data link connector located under the crash pad.
3. | Turn the ignition switch on and power on the scantool.
4. | Read DTCs.
5. | Find and repair the trouble, and clear the DTCs using scantool.
6. | Disconnect the scantool.
7. | Confirm proper system operation :
A. | Turn the ignition switch ON ; the SRS indicator light should be turned on for about six seconds and then to off.
DIAGNOSTIC TROUBLESHOOTING FLOW Verification of Vehicle Repair After a repair, it is essential to verify that the fault has been corrected.
1. | Connect scantool and select "Diagnostic Trouble Codes(DTC)" mode.
2. | Using a scantool, clear the DTC.
3. | Operate the vehicle within DTC Enable conditions in General information.
4. | Are any DTC present ? ▶ Go to the applicable troubleshooting procedure. ▶ System is performing to specification at this time.