| TIBURON(GK) >2008 > G 2.0 DOHC > Restraint > Supplemental Restraint System Control Module (SRSCM) > Occupant Classification Sensor (OCS)>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front seat assembly. (Refer to BD group)
3. | Remove the seat cushion as an assembly. (Refer to BD group)
INSTALLATION
1. | Install the OCS equipped seat cushion. (Refer to BD group)
2. | Install the front seat assembly. (Refer to BD group)
3. | Reconnect the battery negative cable.
4. | After installing OCS, confirm proper system operation : Turm the ignition switch ON, the SRS indicator should be turn on for about six seconds and then off. Telltale lamp will turn on for 4 seconds and be turned off for 4 seconds. After the 8 seconds, it shall remain off if the OCS does not require suppression and the passenger airbag is enabled.
Besure to perform OCS(PODS) rezero with scantool in empty seat condition after replacing OCS equipped seat cushion.