| TIBURON(GK) >2008 > G 2.0 DOHC > Restraint > Supplemental Restraint System Control Module (SRSCM) > Front Impact Sensor (FIS)>Repair procedures |

REMOVAL
• | Removal of the airbag must be performed according to the precautions/ procedures described previously.
• | Before disconnecting the front impact sensor connector, disconnect the front airbag connector(s).
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the front impact sensor.
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the head lamp assembly. (Refer to BE group)
3. | Disconnect the Front Impact Sensor connector.
4. | Loosen the Front Impact Sensor mounting bolts and remove the Front Impact Sensor.
INSTALLATION
• | Do not turn the ignition switch ON and do not contact the battery cable while replacing the front impact sensor.
1. | Install the new Front Impact Sensor with bolts then connect the SRS harness connector to the Front Impact Sensor.
Tightening torque : 0.7 ~ 1.3 kgf.m (7 ~ 13 Nm, 5.2 ~ 9.6 lb.ft)
2. | Install the head lamp assembly. (Refer to BE group)
3. | Reconnect the negative battery cable.
4. | After installing the Front Impact Sensor, confirm proper system operation: Turn the ignition switch ON the SRS indicator light should be turned on for about six seconds and then go off.