| TIBURON(GK) >2008 > G 2.0 DOHC > Body Electrical System > Fuses And Relays > Relay Box (Passenger Compartment)>Components and Components Location |

COMPONENTS
FUSE
NO. | CAPACITY | DESCRIPTION
1 | 20A | Ignition coil (2.7L), Electronic chrome mirror
2 | 20A | AMP
3 | 10A | Back-up lamp switch, Transaxle range switch, Stop lamp switch
4 | 10A | Instrument cluster (Airbag indicator)
5 | 15A | Airbag control module , Seat belt buckle switch
6 | 10A | Mirror defogger
7 | 10A | Hazard lamp relay
8 | 15A | Rear wiper motor, Rear intermittent wiper relay
9 | 10A | Right tail lamps, Glove box lamp
10 | 20A | Front wiper motor, Front wiper relay
11 | 10A | Blower relay, Blower motor
12 | 30A | Defogger relay
13 | 15A | Stop lamp switch, Folding /unfolding relay, Burglar alarm horn relay
14 | 10A | Left tail lamps
15 | 10A | A/C control module, Blower relay
16 | 10A | ECM, Multi gauge unit, TCM, Vehicle speed sensor
17 | 10A | Instrument cluster(Power), Alternator resister, DRL Control module, Pre-excitation resistor
18 | 10A | Room lamp, Clock, Audio, Data link connector, Multi gauge unit
19 | 30A | Power window relay
20 | 15A | Trunk lid switch
21 | 10A | AQS sensor, Head lamp relay, DRL Control module
22 | - | -
23 | 15A | Cigar lighter, Outside mirror switch
24 | 15A | Sunroof , Power door lock/unlock relay
25 | 20A | Seat heater
26 | 10A | ESP/ABS control module
27 | 10A | Audio, Clock