| TIBURON(GK) >2008 > G 2.0 DOHC > Restraint > General Information>Repair procedures |

COMPONENT REPLACEMENT AFTER DEPLOYMENT
Before doing any SRS repairs, use the Hi-Scan Pro to check for DTCs. Refer to the Diagnostic Trouble Code list for repairing of the related DTCs.
When the front airbag(s) deployed after a collision, replace the following items.
- | SRSCM
- | Deployed airbag(s)
- | Deployed seat belt pretensioner(s)
- | Front impact sensors
- | SRS wiring harnesses
- | Inspect the clock spring for heat damage. If any damage found, replace the clock spring.
When the seat belt pretensioner(s) deployed after a collision, replace the following items.
- | Deployed seat belt pretensioner(s)
- | SRSCM
- | Front impact sensors
- | SRS wiring harnesses
When the side/curtain airbag(s) deployed after a collision, replace the following items.
- | SRSCM
- | Deployed airbag(s)
- | Side impact sensor(s) for the deployed side(s)
- | SRS wiring harnesses
After the vehicle is completely repaired, confirm the SRS airbag system is OK.
- | Turn the ignition switch ON, the SRS indicator should come on for about 6 seconds and then go off.