| TIBURON(GK) >2008 > G 2.0 DOHC > Body Electrical System > Sun Roof > Sunroof Motor>Repair procedures |

INSPECTION
1. | Pull down the rear headliner.
2. | Disconnect the motor side connector from the sunroof controller. Remove the sunroof motor after removing 3 screws.
3. | Connect the positive (+) lead from the battery to terminal 2 and the nagative (-) lead to terminal 1, check that the motor turns counterclockwise (moves toward the close and down position).
4. | Reverse the polarity, check that the motor turns clockwise (moves toward the up and open position). If operation is not as specified, replace the motor.