| TIBURON(GK) >2008 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Blower > Blower Resistor>Description and Operation |

DESCRIPTION
- | Rated voltage : DC 12V
- | Rated load : Blower motor
- | Standard test Temp. : 20DEG
- | Operation Temp. : -30DEG ~ +70DEG
- | Resistor off - Time requierment for blower motor locking
Mode | Resistor off time (sec)
1 | 200 ± 30
2 | 100 ± 20
3 | 55 ± 15
CHARACTERISTICS