| TIBURON(GK) >2008 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Air conditioning System > Condenser>Repair procedures |

REPLACEMENT
1. | Recover the refrigerant with a recovery/recycling/charging station.
2. | Remove the coolant reservoir, but do not disconnect the reservoir hose from the coolant reservoir and the radiator.
3. | Remove the bolts(A), then remove the upper mount brackets(B) from the radiator.
4. | Remove the bolts(A), then disconnect the discharge line and condenser line from the condenser. Plug or cap the lines immediately after disconnecting them to avoid moisture and dust contamination.
5. | Remove the bolts, then remove the condenser by lifting it up. Be careful not to damage the radiator and condenser fins when removing the condenser.
6. | Install in the reverse order of removal, and note these items :
A. | If you're installing a new condenser, add refrigerant oil FD46XG.
B. | Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the right O-rings for R-134a to avoid leakage.
C. | Be careful not to damage the radiator and condenser fins when installing the condenser.
D. | Be sure to install the lower mount cushions of condenser securely into the holes.
E. | Charge the system, and test its performance.