| TIBURON(GK) >2008 > G 2.0 DOHC > Body Electrical System > Trip Computer>Description and Operation |

DESCRIPTION
The trip computer displays information related to driving, including distance to empty, average speed and running time on this display. To change the function as described below, push the mode button less than 1 second. ODO meter [1] → Distance to empty [2] → Average speed [3] → Running time [4] → ODO meter [1].
OPERATION
FUNCTION
Item | Function | Detection | Remark
Distance to empty | The estimated distance indication to empty | Fuel sender | 1Km(1mile)
Average speed | The average speed indication since the last driving time reset | Speed sensor | 1Km/h(1MPH)
Running time | The total time traveled since the last driving time reset | Fuel sender | 1Min
Distance to empty mode
1. | Description This mode indicates the estimated distance to empty based on the current fuel in the fuel thank and the amount of fuel delivered to the engine.
2. | Indication range : 50Km ~ 999Km(30miles ~ 999miles)
3. | Indication division : 1Km(mile) When the remaining amount is below 5ℓ, "---" symbol will be displayed during 64sec. When the remaining distance is below 50km(30miles), "---" symbol will be displayed.
4. | Data clear : at battery + off
Average speed mode
1. | Description This mode indicates the estimated speed by the driving distance to the indication timing after reconnecting the batter or resetting the data.
2. | Indication range : 0 Km/h(MPH) ~ 999 Km/h(MPH)
3. | Indication division : 1Km/h(MPH) When the battery is reconnected or the data are reset, "---" symbol will be displayed until the timing.
4. | Indication interval : 10 sec.
5. | Data clear: press the reset button for more than 1 sec. or at first Battery + on
Running time mode
1. | Description This mode indicates the total time traveled since the last driving time reset while the engine is running.
2. | Indication range : 0:00 ~ 99:59
3. | Indication division : 1Min (0:01)
4. | Data clear: press the reset button for more than 1 sec. or Battery +on ※ For removal and installation of trip computer SW, please refer to the instrument cluster.