| TIBURON(GK) >2008 > G 2.0 DOHC > Restraint > Airbag Module > Side Airbag (SAB) Module>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable and wait at least 3 minutes before beginning work.
2. | Remove the front seat assambly.(Refer to BD group)
3. | Remove the seat-back cover.(Refer to BD group)
4. | Loosen the SAB mounting nuts and remove the SAB module.
The removed airbag module should be stored in a clean, dry place with the pad cover face up.
INSTALLATION
Be sure to install the harness wires not to be pinched or interfered with other parts.
• | Do not open the lid of the side airbag cover.
• | Use a new mounting nuts when you replace a side airbag.
• | Make sure that the seat-back cover is installed properly. Improper installation may prevent the proper deployment.
1. | Remove ignition key from the vehicle.
2. | Disconnect the battery negative cable and wait for at least three minutes.
3. | Place a Side Airbag (SAB) on the seat-back frame and tighten the side airbag mounting nuts.
Tightening torque : 1.0 ~ 1.6 kgf.m (10.2 ~ 15.8 Nm, 7.5 ~ 11.7 lb.ft)
4. | Install the new seat-back cover.(Refer to BD group)
5. | Install the seat assembly, then connect the Side Airbag (SAB) harness connector.
6. | Recline and slide the front seat forward fully, make sure the harness wires are not pinched or interfering with other parts.
7. | Reconnect the battery negative cable.
8. | After installing the Side Airbag (SAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.