| TIBURON(GK) >2008 > G 2.0 DOHC > Body Electrical System > Keyless Entry And Burglar Alarm > Transmitter>Repair procedures |

INSPECTION
1. | Check that the red light flickers when the door lock or unlock button is pressed on the transmitter.
2. | Remove the battery and check voltage if the red light doesn't flicker.
Standard voltage : 3V
3. | Replace the transmitter battery with a new one, if voltage is below 3V then try to lock and unlock the doors with the transmitter by pressing the lock or unlock button five or six times.
4. | If the door lock still does not operates, register the transmitter code, then try to lock and unlock the doors.
5. | If the door lock still does not operates, replace the transmitter.
TRANSMITTER CODE REGISTRATION
1. | Connect the DLC cable of hi-scan to the data link connector (16 pins) in driver side crash pad lower panel, turn the power on hi-scan.
2. | Select the vehicle model and then do "CODE SAVING".
3. | After selecting "CODE SAVING" menu, button "ENTER" key, then the screen will be shown as below.
4. | After removing the ignition key from key cylinder, push "ENTER" key to proceed to the next mode for code saving. Follow steps 1 to 3 and then code saving is completed.
Take care when you remove the diagnostic tool connector. Don’t remove it with holding the wiring by hand. Please hold the body of it.