| TIBURON(GK) >2008 > G 2.7 DOHC > Heating,Ventilation, Air Conditioning > Air conditioning System > Triple pressure switch>Description and Operation |

DESCRIPTION
- | Rating load : Inductive loacl DC 12V, 10~250mA
- | Applicable voltage range : DC 8V ~ DC 16V
- | Applicable temperature range : -30°C ~ 120°C
- | Applicable refrigerant : R-134a
- | Insulation resistance : Min. 100MΩ at DC 500V
Pressure | ON | OFF
High | 32.0 ± 2.0 | 26.0 ± 2.0
Low | 2.3 + 0.25 / -0.29 | 2.0 ± 0.2
Medium | 18.0 ± 0.8 | 14.0 ± 1.2
LOW & HIGH
MEDIUM