| TIBURON(GK) >2008 > G 2.7 DOHC > Emission Control System > Crankcase Emission Control System > Positive Crankcase Ventilation (PCV) Valve>Repair procedures |

REMOVAL
1. | Disconnect the vacuum hose from the PCV Valve.
2. | Remove the PCV Valve.
INSTALLATION
Install the PCV valve and tighten to the specified torque.
PCV valve tightening toraue: 7.8 ~ 11.8N•m (0.8 ~ 1.2kgf•m, 5.8 ~ 8.7lbf•ft)
INSPECTION
1. | Remove the PCV valve.
2. | Insert a thin stick(A) into the PCV valve(B) from the threaded side to check that the plunger moves.
3. | If the plunger does not move, the PCV valve is clogged. Clean it or replace.