| TIBURON(GK) >2008 > G 2.7 DOHC > Fuel System > Engine Control System>Troubleshooting |

INSPECTION CHART FOR DIAGNOSTIC TROUBLE CODE
DTC | Description | MIL | Page
P0030 | HO2S Heater Control Circuit (Bank 1 / Sensor 1) | ● |
P0031 | HO2S Heater Circuit low (Bank 1 / Sensor 1) | ● |
P0032 | HO2S Heater Circuit high (Bank 1 / Sensor 1) | ● |
P0036 | HO2S Heater Control Circuit (Bank 1 / Sensor 2) | ● |
P0037 | HO2S Heater Circuit low (Bank 1 / Sensor 2) | ● |
P0038 | HO2S Heater Circuit high (Bank 1 / Sensor 2) | ● |
P0050 | HO2S Heater Control Circuit (Bank 2 / Sensor 1) | ● |
P0051 | HO2S Heater Circuit low (Bank 2 / Sensor 1) | ● |
P0052 | HO2S Heater Circuit high (Bank 2 / Sensor 1) | ● |
P0056 | HO2S Heater Control Circuit (Bank 2 / Sensor 2) | ● |
P0057 | HO2S Heater Circuit low (Bank 2 / Sensor 2) | ● |
P0058 | HO2S Heater Circuit high (Bank 2 / Sensor 2) | ● |
P0101 | Mass or Volume Air Flow Circuit Range / Performance Problem | ● |
P0102 | Mass or Volume Air Flow circuit Low Input | ● |
P0103 | Mass or Volume Air Flow circuit High Input | ● |
P0111 | Intake Air Temperature Sensor 1 Circuit Range / Performance | ● |
P0112 | Intake Air Temperature Sensor 1 Circuit Low Input | ● |
P0113 | Intake Air Temperature Sensor 1 Circuit High Input | ● |
P0116 | Engien Coolant Temperature Circuit Range / Performance | ● |
P0117 | Engine Coolant Temperature Circuit Low Input | ● |
P0118 | Engine Coolant Temperature Circuit Hgih Input | ● |
P0119 | Engine Coolant Temperture Circuit Intermittent | ● |
P0121 | Throttle / Pedal Position Sensor / Switch "A" Circuit Range/Performance | ● |
P0122 | Throttle / Pedal Position Sensor / Switch "A" Circuit Low Input | ● |
P0123 | Throttle / Pedal Position Sensor / Switch "A" Circuit Hgih Input | ● |
P0125 | Insufficient Coolant Temperature for Closed Loop Fuel Control | ● |
P0128 | Coolant Thermostat (Coolant Temp. below Thermostat Regulating Temp.) | ● |
P0130 | HO2S Circuit (Bank 1 / Sensor 1) | ● |
P0131 | HO2S Circuit Low Input (Bank 1 / Sensor 1) | ● |
P0132 | HO2S Circuit High Input (Bank 1 / Sensor 1) | ● |
P0133 | HO2S Circuit Slow Response (Bank 1 / Sensor 1) | ● |
P0134 | HO2S Circuit No Activity Detected (Bank 1 / Sensor 1) | ● |
P0136 | HO2S Circuit (Bank 1 / Sensor 2) | ● |
P0137 | HO2S Circuit Low Input (Bank 1 / Sensor 2) | ● |
P0138 | HO2S Circuit High Input (Bank 1 / Sensor 2) | ● |
P0139 | HO2S Circuit Slow Response (Bank 1 / Sensor 2) | ● |
P0140 | HO2S Circuit No Activity Detected (Bank 1 / Sensor 2) | ● |
P0150 | HO2S Circuit (Bank 2 / Sensor 1) | ● |
P0151 | HO2S Circuit Low Input (Bank 2 / Sensor 1) | ● |
P0152 | HO2S Circuit High Input (Bank 2 / Sensor 1) | ● |
P0153 | HO2S Circuit Slow Response (Bank 2 / Sensor 1) | ● |
P0154 | HO2S Circuit No Activity Detected (Bank 2 / Sensor 1) | ● |
P0156 | HO2S Circuit Malfunction (Bank 2 / Sensor 2) | ● |
P0157 | HO2S Circuit Low Input (Bank 2 / Sensor 2) | ● |
P0158 | HO2S Circuit High Input (Bank 2 / Sensor 2) | ● |
P0159 | HO2S Circuit Slow Response (Bank 2 / Sensor 2) | ● |
P0160 | HO2S Circuit No Activity Detected (Bank 2 / Sensor 2) | ● |
P0170 | Fuel Trim (Bank 1) | ● |
P0171 | System Too Lean (Bank 1) | ● |
P0172 | System Too Rich (Bank 1) | ● |
P0173 | Fuel Trim (Bank 2) | ● |
P0174 | System Too Lean (Bank 2) | ● |
P0175 | System Too Rich (Bank 2) | ● |
P0230 | Fuel Pump Circuit Malfunction | ▲ |
P0261 | Cylinder 1 - Injector Circuit Low | ● |
P0262 | Cylinder 1 - Injector Circuit High | ● |
P0264 | Cylinder 2 - Injector Circuit Low | ● |
P0265 | Cylinder 2 - Injector Circuit High | ● |
P0267 | Cylinder 3 - Injector Circuit Low | ● |
P0268 | Cylinder 3 - Injector Circuit High | ● |
P0270 | Cylinder 4 - Injector Circuit Low | ● |
P0271 | Cylinder 4 - Injector Circuit High | ● |
P0273 | Cylinder 5 - Injector Circuit Low | ● |
P0274 | Cylinder 5 - Injector Circuit High | ● |
P0276 | Cylinder 6 - Injector Circuit Low | ● |
P0277 | Cylinder 6 - Injector Circuit High | ● |
P0300 | Random / Multiple Cylinder Misfire Detected | ● |
P0301 | Cylinder 1 - Misfire detected | ● |
P0302 | Cylinder 2 - Misfire detected | ● |
P0303 | Cylinder 3 - Misfire detected | ● |
P0304 | Cylinder 4 - Misfire detected | ● |
P0305 | Cylinder 5 - Misfire detected | ● |
P0306 | Cylinder 6 - Misfire detected | ● |
P0315 | Segment Time Acquisition Incorrect | ▲ |
P0325 | Knock Sensor 1 Circuit | ▲ |
P0330 | Knock Sensor 2 Circuit | ▲ |
P0335 | Crankshaft Position Sensor A Circuit | ● |
P0340 | Camshaft Position Sensor A Circuit Malfuntion (Signal Sensor) | ● |
P0350 | Ignition Coil Primary / Secondary Circuit | ▲ |
P0351 | Ignition Coil 'A' Primary / Secondary Circuit | ▲ |
P0352 | Ignition Coil 'B' Primary / Secondary Circuit | ▲ |
P0353 | Ignition Coil 'C' Primary / Secondary Circuit | ▲ |
P0354 | Ignition Coil 'D' Primary / Secondary Circuit | ▲ |
P0355 | Ignition Coil 'E' Primary / Secondary Circuit | ▲ |
P0356 | Ignition Coil 'F' Primary / Secondary Circuit | ▲ |
P0420 | Catalyst System Efficiency below Threshold (Bank 1) | ● |
P0430 | Catalyst System Efficiency below Threshold (Bank 2) | ● |
P0441 | Evap. Emission System Incorrect Purge Flow | ● |
P0442 | Evap. Emission System - Leak Detected (Small Leak) | ● |
P0444 | Evap. Emission System - Purge Ctrl. Valve Circuit Open | ● |
P0445 | Evap. Emission System - Purge Ctrl. Valve Circuit Shoted | ● |
P0447 | Evap. Emission System - Vent Control Circuit Open | ● |
P0448 | Evap. Emission System - Vent Control Circuit Shorted | ● |
P0449 | Evap. Emission System - Vent valve / Solenoid circuiit | ● |
P0451 | Evap. Emission System - Pressure Sensor Rage / Performance | ● |
P0452 | Evap. Emission System - Pressure Sensor Low Input | ● |
P0453 | Evap. Emission System - Pressure Sensor High Input | ● |
P0454 | Evap. Emission System - Pressure Sensor Intermittent | ● |
P0455 | Evap. Emission System - Leak Detected (Large Leak) | ● |
P0456 | Evap. Emission System - Leak Detected (Very small Leak) | ● |
P0461 | Fuel Level Sensor "A" Circuit Range / Performance | ▲ |
P0462 | Fuel Level Sensor "A" Circuit Low Input | ▲ |
P0463 | Fuel Level Sensor "A" Circuit Hign Input | ▲ |
P0464 | Fuel Level Sensor "A" Circuit Intermittent | ▲ |
P0501 | Vehicle Speed Sensor "A" Range / Performancd | ● |
P0505 | Idle Air Control System | ● |
P0506 | Idle Air Control System - RPM lower than expected | ● |
P0507 | Idle Air Control System - RPM higher than expected | ● |
P0551 | Power Steering Pressure Sensor / Switch Circuit Range / Performance | ▲ |
P0560 | System Voltage | ● |
P0562 | System Voltage Low | ● |
P0563 | System Voltage High | ● |
P0605 | Internal Control Module Read Only Memory (ROM) Error | ● |
P0630 | VIN not Programmed or Incompatible - ECM/PCM | ● |
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ▲ |
P0700 | TCM Request for MIL On | ● |
P1505 | Idle Charge Actuator Signal Low of Coil #1 | ● |
P1506 | Idle Charge Actuator Signal High of Coil #1 | ● |
P1507 | Idle Charge Actuator Signal Low of Coil #2 | ● |
P1508 | Idle Charge Actuator Signal High of Coil #2 | ● |
U0101 | Serial Communication Problem with TCM (Timeout) | ● |
- | ● : MIL ON & FAULT CODE MEMORY
- | ▲ : MIL OFF & FAULT CODE MEMORY