| TIBURON(GK) >2008 > G 2.7 DOHC > Brake System > Brake Warning System > Parking Brake Assembly>Repair procedures |

REMOVAL
• | The parking brake cables must not be bent or distorted. This will lead to stiff operation and premature failure.
• | Refer to the component as needed during this procedure.
Rear disc brake
1. | Release the parking brake lever fully, and remove the parking cable clip (A) from the parking brake cable.
2. | Disconnect the parking brake cable (B) from the lever (C).