| TIBURON(GK) >2008 > G 2.7 DOHC > Body Electrical System > Sun Roof > Sunroof Relay>Repair procedures |

INSPECTION
1. | Pull down the rear headliner.
2. | Disconnect the sunroof switch side connector from the sunroof controller.
3. | Inspect the connectors on the wire harness side from the controller, as shown in the table.
Connector | Tester connection | Condition | Specified condition
M97 | 1-Ground | Constant | Continuity
2-Ground | Sunroof switch is in the close position | Continuity
3-Ground | Sunroof switch is in the open position | Continuity
4-Ground | Constant | Battery voltage
6-Ground | Ignition switch ON | Battery voltage
7-Ground | Sunroof switch is in the tilted up position | Continuity
8-Ground | Sunroof switch is in the tilted down position | Continuity
M99 | 3-Ground | Constant | Continuity
1(+) ~ 2(-) | Apply the battery voltage to the terminal No.1 and ground to terminal No.2 | Motor turns clockwise
1(-) ~ 2(+) | Apply the battery voltage to the terminal No.2 and ground to terminal No.1 | Motor turns counter-clockwise