| TIBURON(GK) >2008 > G 2.7 DOHC > Suspension System > Tire Pressure Monitoring System > TPMS Receiver>Repair procedures |

REPLACEMENT
When the receiver first arrives for replacement:
1) | It will be in Virgin State.
2) | It will not be configured for any specific platform.
3) | It will not have any sensor ID's memorized.
• | It is important to make sure that the correct receiver is used to replace the faulty part i.e. it must be Low Line and not High Line in order to have the correct inflation warning thresholds set.
• | Receiver software version must be 8.4 or higher. (Receiver software can be checked with hand tool.)
1. | Disconnect vehicle battery.
2. | Remove faulty part and fit bracket assembly to new part.
3. | Secure new part to vehicle and fit connector.
4. | Re-connect battery and turn Ignition on.
5. | Check that DTC flash rate matches Virgin State indication.
6. | Connect 'TPMS exciter' to the diagnostic connector.
7. | Write vehicle name to receiver. receiver will now automatically update monitoring parameters.
8. | Read sensor's ids with the 'TPMS exciter'. (Refer to 'SENSOR INITIATING PROCEDURE')
9. | Register sensor's ids to receiver.
10. | Register VIN number of the vehicle.(17 digits)
11. | Change receiver state from Virgin to Normal.
12. | Disconnect diagnostic link.
13. | Turn ignition off for approximately 10 seconds then turn it back on and check that Normal State is now indicated.