| TIBURON(GK) >2008 > G 2.7 DOHC > Restraint > Supplemental Restraint System Control Module (SRSCM) > Side Impact Sensor (SIS)>Repair procedures |

REMOVAL
• | Removal of the airbag must be performed according to the precautions/procedures described previously.
• | Before disconnecting the side impact sensor connector(s), disconnect the side airbag connector(s).
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the side impact sensor.
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front seat. (Refer to BD group)
3. | Remove the door scuff trim and center pillar trim.
4. | Remove the floor carpet.
5. | Disconnect the Side Impact Sensor connector.
6. | Remove the SIS mounting bolt then remove the Side Impact Sensor. [DEPOWERED] [ADVANCED]
INSTALLATION
• | Do not turn the ignition switch ON and do not connect the battery cable while replacing the side impact sensor.
1. | Install the new Side Impact Sensor with the bolt then connect the SRS harness connector to the Side Impact Sensor.
Tightening torque : [ADVANCED] 0.7 ~ 1.3 kgf.m (7 ~ 13 Nm, 5.2 ~ 9.6 lb.ft) [DEPOWERED] 0.6 ~ 0.8 kgf.m (6 ~ 8 Nm, 4.4 ~ 5.9 lb.ft)
2. | Install the following parts. (Refer to BD group)
A. | Door scuff trim, Center pillar trim
3. | Reconnect the negative battery cable.
4. | After installing the Side Impact Sensor, confirm proper system operation: Turn the ignition switch ON, the SRS indicator light should be turned on for about six seconds and then go off.