| TIBURON(GK) >2008 > G 2.7 DOHC > Restraint > Airbag Module > Passenger Airbag (PAB) Module>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable and wait for at least three minutes before beginning work.
2. | Remove the glove box. (Refer to BD group)
3. | Disconnect the PAB connector and remove the PAB mounting bolts. (Refer to BD group) [DEPOWERED] [ADVANCED]
4. | Remove the crash pad. (Refer to BD group)
Replace the crash pad which is damaged while PAB is deployed.
5. | Remove the mounting nuts from the crash pad. Then remove the passenger airbag.
The removed airbag module should be stored in a clean, dry place with the pad cover face up.
INSTALLATION
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Place a Passenger Airbag (PAB) on the crash pad and tighten the Passenger Airbag (PAB) mounting nuts.
4. | Install the crash pad. (Refer to BD group)
5. | Tighten the PAB mounting bolts.
Tightening Torque : 0.7 ~ 1.1 kgf.m (7 ~ 11 N.m, 5.2 ~ 8.1 lb.ft)
6. | Connect the Passenger Airbag (PAB) harness connector to the SRS main harness connector.
7. | Reinstall the glove box. (Refer to BD group)
8. | Reconnect the battery negative cable.
9. | After installing the Passenger Airbag (PAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.