| TIBURON(GK) >2008 > G 2.7 DOHC > Driveshaft and axle > Rear Axle Assembly > Rear Hub - Carrier>Repair procedures |

REMOVAL
1. | Remove the rear wheel speed sensor (for vehicles equipped with ABS(Anti-lock Brake System)).
When removing the speed sensor from the adapter, be careful so that the end of the pole piece doesn't strike teeth on the rotor or other components.
2. | Remove the caliper assembly and suspend it with a wire.
3. | Remove the brake disc.
4. | Remove the hub cap, wheel bearing nut and tongue washer.
5. | Remove the hub assembly.
• | The rear hub assembly should not be disassembled.
• | (For vehicles equipped with ABS(Anti-lock Brake System)) Care must be taken not to scratch or damage the teeth of the rotor. The rotor must never be dropped. If the teeth of the rotor are chipped, it results in deformation of the rotor. It will make it impossible to detect the wheel rotation speed accurately and to operate the system normally.
INSTALLATION
1. | After tightening the flange nut, caulk the concave portion of the spindle by crimping the nut.
Replace the flange nut with new ones after removal.
2. | Installation of the rear speed sensor (For vehicles equipped with ABS(Anti-lock Brake System)) : Insert a feeler gauge into the space between the pole piece of the speed sensors and the rotor teeth surface, and then tighten the speed sensors at the position where the clearance at all places is within the standard value.
Standard value Clearance : 0.2~1.3 mm (0.008~0.051 in.)
3. | Install the hub cap.
INSPECTION
1. | Check the oil seal for cracks or damage.
2. | Check the rear hub bearing for wear or damage.
3. | Check the rear rotor for chipped teeth.
4. | Check the rear carrier for cracks.