| TIBURON(GK) >2008 > G 2.7 DOHC > Body Electrical System > Power Door Locks > Power Door Lock Actuators>Repair procedures |

INSPECTION
DOOR LOCK ACTUATOR INSPECTION
1. | Remove the door trim panel.
2. | Disconnect the 6P connector from the actuator.
3. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.
DOOR LOCK SWITCH INSPECTION
1. | Remove the door trim panel.
2. | Disconnect the 6P connector from the actuator.
3. | Check for continuity between the terminals in each switch position according to the table.