| TUCSON(LM) >2010 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > Cluster Ion Generator>Repair procedures |

Inspection
1. | Press the OFF switch more then 4 times within 2 seconds while pressing the MODE switch.
Display | Fail description
00 | Normal
50 | Cluster ion generator fault
* Diagnostic procedure refer to DTC code.
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the extension cover (A).
3. | Disconnect the damper (A) from the glove box (B).
4. | Remove the glove box lift (A).
5. | Disconnect the pine (A), then remove the glove box (B).
6. | Remove the crash pad passenger panel(A).
7. | Remove the glove box housing (A).
8. | Remove the shower duct (A).
9. | Loosen the screws and then remove the cluster ionizer (A).
10. | Installation is the reverse order of removal.