| TUCSON(LM) >2010 > G 2.0 DOHC > Body Electrical System > Lighting System > High Mounted stop lamp>Repair procedures |

Removal
High Mounted Stop Lamp
1. | Disconnect the negative (-) battery terminal.
2. | Remove the tailgate trim. (Refer to the BD group - "Tailgate")
3. | Remove the spoiler. (Refer to the BD group - "Tailgate")
4. | Remove the high mounted stop lamp assembly (A) after loosening the nuts and washer nozzle (B).
Installation
1. | Install the high mounted stop lamp and washer nozzle.
2. | Install the spoiler and tailgate trim.