| TUCSON(LM) >2010 > G 2.0 DOHC > Suspension System > Rear Suspension System > Trailing Arm>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Loosen the nuts & bolts and then remove the trailing arm(A) with the rear axle.
Tightening torque Trailing arm : 34.3 ~ 53.9N.m(3.5 ~ 5.5Kgf.m, 25.3 ~ 39.8lb-ft) Parking brake cable bracket : 6.9 ~ 10.8N.m(0.7 ~ 1.1Kgf.m, 5.1 ~ 8.0lb-ft)
[2WD] [4WD]
3. | Loosen the parking brake cable bracket bolt(A) & height sensor bracket bolt(B). [2WD/4WD]
4. | Loosen the mounting bolt and then remove the trailing arm(A) with the frame.
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.8lb-ft)
5. | Installation is the reverse of removal.