| TUCSON(LM) >2010 > G 2.0 DOHC > Restraint > General Information>Repair procedures |

Component Replacement After Deployment
Before doing any SRS repairs, use the GDS Pro to check for DTCs. Refer to the Diagnostic Trouble Code list for repairing of the related DTCs.
When the front airbag(s) deployed after a collision, replace the following items.
- | SRSCM
- | Deployed airbag(s)
- | Seat belt pretensioner(s)
- | Front impact sensors
- | SRS wiring harnesses
- | Inspect the clock spring for heat damage. If any damage found, replace the clock spring.
When the side/curtain airbag(s) deployed after a collision, replace the following items.
- | SRSCM
- | Deployed airbag(s)
- | Side impact sensor(s) for the deployed side(s)
- | SRS wiring harnesses
After the vehicle is completely repaired, confirm the SRS airbag system is OK.
- | Turn the ignition switch ON; the SRS indicator should come on for about six seconds and then go off.