| TUCSON(LM) >2010 > G 2.0 DOHC > Body (Interior and Exterior) > Interior > Interior Trim>Repair procedures |

Replacement
Door Scuff Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the door scuff trim (A). [Front] [Rear]
2. | Installation is the reverse of removal.
• | Replace any damage clips.
Front Pillar Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | After loosening the mounting screw, then remove the front pillar trim (A).
2. | Installation is the reverse of removal.
• | Replace any damage clips.
Cowl Side Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the front door scuff trim.
2. | Remove the hood latch release handle. (Refer to the BD group - "Hood")
3. | Remove the cowl side trim (A).
4. | Installation is the reverse of removal.
• | Replace any damage clips.
Center Piller Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the front door scuff trim and rear door scuff trim.
2. | After loosening the mounting bolt, then remove the front seat belt lower anchor (A).
3. | Remove the center lower pillar trim (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb.ft)
4. | Remove the cap, loosen the mounting bolts.
5. | Remove the center upper pillar trim (A).
6. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Pillar Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the rear seat. (Refer to the BD group - "Rear seat")
2. | Remove the rear door scuff trim.
3. | Detach the clips and then remove the transverse trim (A).
4. | After loosening the mounting bolt, then remove the rear sent belt lower anchor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb.ft)
5. | After loosening the mounting bolts, then remove the rear seat bracket (A).
6. | Using a screwdriver, remove the lamp (A).
7. | Disconnect the connector (B).
8. | After loosening the mounting screws, then remove the luggage side trim (C).
9. | Disconnect the connector (A).
10. | After loosening the mounting bolt and screws, then remove the rear pillar trim (A).
11. | Installation is the reverse of removal.
• | Replace any damage clips.
Luggage Side Trim Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the rear seat. (Refer to the BD group - "Rear seat")
2. | Remove the transverse trim.
3. | After loosening the mounting screws, then remove the luggage side trim.
4. | Installation is the reverse of removal.
• | Replace any damage clips.
1. Luggage side trim (LH) 2. Luggage side trim (RH) 3. Transverse trim | 4. Luggage board 5. Speaker cover trim 6. Triangle