| TUCSON(LM) >2010 > G 2.0 DOHC > Body Electrical System > Lighting System > Room Lamp>Repair procedures |

Inspection
1. | Remove the room lamp assembly connector (A) then check for continuity between terminals.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Detach the lamp lens (A) from the room lamp with a flat-tip screwdriver.
Push the lens as shown arrow direction. Take care not to damage the part (B).
3. | Loosen the fixing screw (2EA).
4. | Remove the room lamp assembly (A) after disconnecting the connector (B).
Installation
1. | Install the room lamp assembly after connecting the lamp connector.
2. | Install the lamp lens after assembling the bulb.