| TUCSON(LM) >2010 > G 2.0 DOHC > Restraint > Airbag Module > Passenger Airbag (PAB) Module>Repair procedures |

Removal
1. | Disconnect the battery negative cable and wait for at least three minutes before beginning work.
2. | Remove the glove box housing. (Refer to the Body group- crash pad).
3. | Disconnect the passenger airbag connector and remove the PAB mounting bolt.
4. | Remove the crash pad. (Refer to the Body group- crash pad).
Replace the crash pad which is damaged while PAB is deployed.
5. | Remove the heater duct from the crash pad.
6. | Remove the mounting nuts(4EA) from the crash pad. Then remove the passenger airbag.
The removed airbag module should be stored in a clean, dry place with the airbag cushion up.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable from battery and wait for at least three minutes before beginning work.
3. | Place a passenger airbag on the crash pad and tighten the passenger airbag mounting bolts.
Tightening torque : 5.9 ~ 6.9 Nm (0.6 ~ 0.7 kgf.m, 4.3 ~ 5.1 lb.ft)
4. | Install the heater duct to the crash pad.
5. | Install the crash pad. (Refer to the Body group- crash pad)
6. | Tighten the passenger airbag mounting bolt.
Tightening torque : 18.6 ~ 26.5 Nm (1.9 ~ 2.7 kgf.m, 13.7 ~ 19.2 lb.ft)
7. | Connect the passenger airbag harness connector to the SRS main harness connector.
8. | Reinstall the glove box. (Refer to the Body group- crash pad)
9. | Reconnect the battery negative cable.
10. | After installing the passenger airbag (PAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.