| TUCSON(LM) >2010 > G 2.0 DOHC > Suspension System > Rear Suspension System > Rear Lower Arm>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Loosen the nut and then remove the rear stabilizer link(B) with the rear lower arm(A).
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.8lb-ft)
3. | Loosen the bolt & nut and then remove the rear lower arm(A) with the rear axle.
Tightening torque : 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft)
4. | Loosen the bolt & nut and then remove the rear lower arm(B) with the sub frame(A).
Tightening torque : 107.9 ~ 117.7N.m(11.0 ~ 12.0Kgf.m, 79.6 ~ 86.8lb-ft)
5. | Installation is the reverse of removal.
6. | Check the alignment. (Refer to 'Tires/Wheels - alingment')
Inspection
1. | Check the bushing for wear and deterioration.
2. | Check the rear lower arm for deformation.
3. | Check the coil spring and spring pad for deterioration and deformation.
4. | Check for all bolts and nut.