| TUCSON(LM) >2010 > G 2.0 DOHC > Manual Transaxle System > Manual Transaxle System>Repair procedures (M5GF1) |

Service Adjustment Procedure
Transmission Oil Inspection And Replacement
1. | After parking the vehicle on a plain, stop the engine.
2. | After removing the oil filler plug and washer, inspect the manual transaxle fluid condition and quantity.
3. | If the manual transaxle fluid is contaminated, drain it out by removing the oil drain plug.
4. | Tighten the new oil drain plug and feed manual transaxle fluid to a proper level.
Tightening torque : 29.4~34.4 N.m(3.0~3.5kgf.m, 21.7~25.3lb-ft) Oil type: SAE75W/85 or API GL-4 Oil quantity: 2.1L (0.14 U.S.gal., 0.55 U.S.qt., 0.46 lmp.qt.)
5. | Retighten the oil filler plug with a new washer.
Tightening torque : 29.4~34.4 N.m(3.0~3.5kgf.m, 21.7~25.3lb-ft)
Back Up Lamp Switch Inspection
1. | Disconnect the back up lamp switch connector(A).
2. | Inspect the continuity of the switch. When the shift lever is located in reverse range, it should be applied an electric current.
3. | Replace the back up lamp switch, if necessary.
Tightening torque : 29.4~34.4 N.m(3.0~3.5kgf.m, 21.7~25.3lb-ft)