| TUCSON(LM) >2010 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > General Information>Specifications |

Specification
Air Conditioner
Item | Specification
Compressor | Type | DVE16
Oil type & Capacity | PAG OIL 120±10cc (4.2±0.35 OZ.)
Pulley type | 6PK-TYPE
Displacement | 160cc/rev
Condenser | Heat rejection | 14,000 ±5% kcal/hr
A/C Pressure transducer | The method to measure the pressure | Voltage= 0.00878835 * Pressure (psig) + 0.5
Expansion valve | Type | Block type
Refrigerant | Type | R-134a
Capacity [oz.(g)] | 510±25 (17.9±0.88)
Blower Unit
Item | Specification
Fresh and recirculation | Operating method | Actuator
Blower | Type | Sirocco
Speed step | Auto + 8 speed (Automatic), 1~4speed (Manual)
Speed control | Power mosfet (Auto)
Air filter | Type | Particle filter
Heater And Evaporator Unit
Item | Specification
Heater | Type | Pin & Tube type
Heating capacity | 4,550 - 5% kcal/hr
Mode operating method | Actuator
Temperature operating method | Actuator
Evaporator | Temperature control type | Evaporator temperature sensor
A/C ON/OFF [°C(°F)] | ON : 1.5 ± 0.3 (34.7 ± 32.5) OFF: -0.5 ± 0.3 (31.1 ± 32.5)