| TUCSON(LM) >2010 > G 2.0 DOHC > Manual Transaxle System > General Information>Specifications (M5GF1) |

Specifications
Manual transaxle type | M5GF1
Engine type | Gasoline 2.0
Gear ratio | 1st | 3.636
2nd | 2.080
3rd | 1.333
4th | 1.061
5th | 0.821
Reverse | 3.455
Final gear ratio | 4.533
T/M oil capacity ※ | 2.1L (0.14 U.S.gal., 0.55 U.S.qt., 0.46 lmp.qt.)
※ The quantity in the chart above is for the reference. The actual filling quantity of the automatic transaxle fluid must be set according to 'INSPECTION' or 'REPLACEMENT' procedure of the manual transaxle fluid.
Recommended transaxle oil | SAE75W/85 or API GL-4
Check&Replenishment | Every 30 months or every 60,000km
Replacement | Private use | Normal use | No service required
Severe use(※) | Every 120,000 Km
Business use
※ Severe use(marked '※') is defined as:
1. | Driving on rough road(bumpy road, gravel road, snowy road, unpaved road etc.).
2. | Driving on mountain road, ascent/descent.
3. | Repetition of short distance driving.
4. | More than 50% operation in heavy city traffic during hot weather above 32°C(89.6°F).
5. | Police car, Taxi, Commercial type operation or trailer towing, etc.
Lubricants
Item | Lubricant | Quantity
Transaxle input shaft splin | CASMOLY L9508 | 0.2 gr.
Transaxle case gasket | LOCTITE 587 | As required
Tightening Torques
Item | N.m | kgf.m | lb-ft
Magnetic plug | 29.4~34.3 | 3.0~3.5 | 21.7~25.3
Shift control cable bracket | 19.6~26.5 | 2.0~2.7 | 4.5~19.5
Oil filler plug | 34.3~44.1 | 3.5~4.5 | 25.3~32.6
Idler shaft bolt | 34.3~41.2 | 3.5~4.2 | 25.3~30.4
Back up lamp switch | 29.4~34.3 | 3.0~3.5 | 21.7~25.3
Vehicle speed sensor | 2.9~3.9 | 0.3~0.5 | 2.2~3.6
Transaxle mounting bracket assembly | 59.2~78.9 | 6.0~8.0 | 43.6~58.2
Transaxle upper mounting bolt | 42.2~53.9 | 4.3~5.5 | 31.1~39.8
Transaxle lower mounting bolt | 42.2 ~ 48.1 42.2 ~ 53.9 | 4.3 ~ 4.9 4.3 ~ 5.5 | 31.1 ~ 35.4 31.1 ~ 39.8