| TUCSON(LM) >2010 > G 2.0 DOHC > Body Electrical System > Back View Camera System>Repair procedures |

Removal
1. | Remove the tailgate trim in the trunk after removing the screws and clips. (Refer to the BD group - "Tailgate")
2. | Remove the tailgate garnish (A) after disconnecting the connector and removing the nuts.
3. | Remove the back view camera (A) after loosening the screws (2EA).
4. | Disconnect the connector (A), and then remove the back view camera module (B).
Installation
1. | Install the back view camera.
2. | Install the tailgate garnish and triPm.