| TUCSON(LM) >2010 > G 2.0 DOHC > Body Electrical System > Hands Free System>Description and Operation |

Function
Bluetooth Audio System
Bluetooth You can use a Bluetooth device in your car to make a hands-free phone call or to stream music onto your in-car speakers (via this Head Unit). This Head Unit supports HFP, A2DP and AVRCP connection.
Advanced Audio Distribution Profile (A2DP)
This profile defines how high quality audio(stereo or mono) can be streamed from one device to another over a Bluetooth connection. For example: music streamed from a mobile phone to a wireless headset or caraudio.
Audio/Video Remote Control Profile (AVRCP)
This profile is designed to provide a standard interface to control TVs, Hi-fi equipment,etc. to allow a single remote control (or other device) to control all of the A/V equipment to which a user has access. It may be used inconcert with A2DP or VDP.
Hands-Free Profile (HFP)
This is commonly used to allow car handsfree kits to communicate with mobile phones in the car.
Notes for mobile phones
Some functions (e.g. starting of speech recognition) are not supported by all mobile phones. We cannot guarantee that all functions described will be supported by all mobile phones with Bluetooth.
New device
This function allows you to add a new phone to the Head Units Bluetooth Device List. Maximum of 5 devices can be added to the list. If the list is full, the oldest device will be replaced by the newly added Bluetooth device, based on last pairing date. Voice Recognition Activation
• | The voice recognition engine containedin the Bluetooth System can be activatedin the following conditions : - Button Activation The voice recognition system will beactive when the button is pressed and after the sound of a Beep. - Active Listening The voice recognition system will beactive for a period of time when the Voice Recognition system has askedfor a customer response.
• | The system can recognize single digits from zero to nine while number greaterthan ten will not be recognized.
• | If the command is not recognized, the system will announce "Pardon" or Noinput voice signal from microphone. (Noresponse)
• | The system shall cancel voice recogntionmode in following cases : When pressing the button and saying cancel following the beep. When not making a call and pressing the button. When voice recognition has failed 3 consecutive times.
• | At any time if you say "help", the system will announce what commands are available.
Menu tree