| TUCSON(LM) >2010 > G 2.0 DOHC > Body Electrical System > Indicators And Gauges>Troubleshooting |

Troubleshooting
Symptom | Possible cause | Remedy
Speedometer does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Speedometer faulty | Check speedometer
CAN line faulty | Check the EMS
Wiring or ground faulty | Repair if necessary
Tachometer does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Tachometer faulty | Check tachometer
CAN line faulty | Check the EMS
Wiring or ground faulty | Repair if necessary
Fuel gauge does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Fuel gauge faulty | Check gauge
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Low fuel warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Water temperature gauge does not operate | Cluster fuse (10A) blown | Check for short and replace fuse
Water temperature gauge faulty | Check gauge
Water temperature sender faulty | Check sender
CAN line faulty | Check the EMS
Wiring or ground faulty | Repair if necessary
Oil pressure warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Oil pressure switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Parking brake warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Brake fluid level warning switch faulty | Check switch
Parking brake switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Open door warning lamp and tailgate warning lamp do not light up | Memory fuse (15A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Door switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Seat belt warning lamp does not light up | Cluster fuse (10A) blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Seat belt switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Speedometer and odometer does not operate | CAN line faulty | Check the ABS ECU
Wheel speed sensor faulty | Check the wheel speed sensor