| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Button Engine Start System > Start/Stop Button>Repair procedures |

Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the left air vent. (Refer to the BD group - "Crash pad")
3. | Disconnect the connector (A).
4. | Remove the start/stop button (A) after loosening the mounting screws.
Installation
1. | Install the start/stop button.
2. | Install the left air vent.