| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Lighting System > Front Fog Lamps>Repair procedures |

Inspection
Front Fog Lamp Switch
1. | With the fog lamp switch in each position, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the multifunction switch.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front bumper. (Refer to the BD group - "Front bumper")
3. | Remove the front fog lamp (A) by turning in the counterclockwise direction after disconnecting the connector.
4. | Remove the front fog lamp (A) after loosening the screws.
Installation
1. | Install the front fog lamp bulb.
2. | Connect the front fog lamp connector.
3. | Install the front bumper.