| TUCSON(LM) >2010 > G 2.4 DOHC > Fuel System > Fuel Delivery System > Fuel Pump>Repair procedures |

Removal
1. | Release the residual pressure in fuel line (Refer to “Release Residual Pressure in Fuel Line” in this group).
2. | Remove the rear seat (Refer to “Seat” in BD group).
3. | Remove the fuel pump service cover (A).
4. | Disconnect the fuel pump connector (A) and the fuel tank pressure sensor connector (B).
5. | Disconnect the fuel feed tube quick connector (C) and the vapor tube quick-connector (D).
6. | Remove locking ring (A) by using the special service tool (B) [No.:09310-2S200].
Fuel Pump locking ring loosening torque: Min. 68.65 M.m (Min. 7 kgf.m, Min. 50.6 lb-ft)
7. | Remove the fuel pump from the fuel tank.
Installation
1. | Installation is reverse of removal.
Be careful of fuel pump direction when installing (Refer to the groove in the fuel tank).