| TUCSON(LM) >2010 > G 2.4 DOHC > Body (Interior and Exterior) > Bumper > Rear Bumper>Repair procedures |

Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not bend or scratch the cover and other parts.
1. | After loosening the mounting screws, then remove the rear combination lamp (A).
2. | Push the lock pin, disconnect the connector (B).
3. | After loosening the rear bumper side's mounting screw and clips, then disconnect the side's.
4. | Loosen the mounting bolts.
5. | Push the lock pin, disconnect the rear bumper main connector (B).
6. | After loosening the mounting screws and clips, then remove the rear bumper (A).
7. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.