| TUCSON(LM) >2010 > G 2.4 DOHC > Suspension System > Rear Suspension System > Rear Assist Arm>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Remove the sprit pin and castle nut or bolt and then disconnect the rear assist arm(A) from the rear axle.
Tightening torque : 2WD 44.1 ~ 53.9N.m(4.5 ~ 5.5Kgf.m, 32.5 ~ 39.8lb-ft) 4WD 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft)
[2WD] [4WD]
3. | Loosen the bolt & nut and then remove the rear assist arm(A) with the sub frame.
Tightening torque : 107.9 ~ 117.7N.m(11.0 ~ 12.0Kgf.m, 79.6 ~ 86.8lb-ft)
[2WD] [4WD]
4. | Installation is the reverse of removal.
5. | Check the alignment. (Refer to 'Tires/Wheels - alingment')
Inspection
1. | Check the bushing for wear and deterioration.
2. | Check the rear assist arm for deformation.
3. | Check ball joint for damage.
4. | Check for the all bolts and nuts.