| TUCSON(LM) >2010 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > In car sensor>Repair procedures |

Inspection
1. | Ignition "ON"
2. | Blow air with changing temperature to the in car sensor air inlet. Measure sensor resistance between 1 and 2 terminals.
1. Sensor Ground | 2. Incar Sensor Signal
Specification
Temperature [°C(°F)] | Resistance between terminals 1and 2 (kΩ)
-20(-4) | 290.21
-10(14) | 165.6
0 (32) | 97.83
10(50) | 59.67
20(68) | 37.48
30(86) | 24.17
40(104) | 15.98
50(122) | 10.81
In car sensor is negative type thermistor that resistance will rise with lower temperature, and reduce with higher temperature.
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the right center air vent and then disconnect the incar sensor connector (A).
3. | Remove the incar sensor (B) from center air vent.
4. | Installation is the reverse order of removal.