| TUCSON(LM) >2010 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Blower > Climate Control Air Filtar>Repair procedures |

Replacement
1. | Remove the right extension cover (A).
2. | Disconnect the damper (A) from the glove box (B).
3. | Remove the glove box lift (C).
4. | Remove the filter cover (A) with pushing the knob.
5. | Replace the air filter (B), install it after making sure of the direction of air filter.
In case of driving in an air-polluted area or rugged terrain, check and replace the air filter as frequently as possible.