| TUCSON(LM) >2010 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > Ambient Sensor>Description and Operation |

Description
1. | The ambient temperature sensor is located at the front of the condenser and detects ambient air temperature. It is a negative type thermistor; resistance will increase with lower temperature, and decrease with higher temperatures.
2. | The sensor output will be used for discharge temperature control, temperature regulation door control, blower motor level control, mix mode control and in-car humidity control.
If the ambient temperature is below 2.0°C (35.6°F), the A/C compressor will be stopped. The compressor will be operated by manual operating.