| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Audio > AUX(Auxiliary) Jack>Repair procedures |

Removal
1. | Remove the floor console upper cover (A) using the appropriate tool.
2. | Remove the seat heater switch module (A).
Take care not to damage the hook when removing the switch.
3. | Disconnect the connectors (A) from the seat heater switch module.
4. | Remove the Multimedia Jack (A) from the seat heater switch module after pressing the hooks.
Installation
1. | Install the multimedia jack.
2. | Connect the AUX jack connector.
3. | Install the center console.
4. | Install the console upper cover.
5. | Install the shift lever knob.
Make sure the Aux connector and the console connectors are plugged in properly.