| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > BCM (Body Control Module) > Body Control Module (BCM)>Specifications |

Specifications
Electrical Performance
Item | Requirement | Remark
Rated voltage | DC 12V |
Operating voltage range | DC 9 ~ 16V | Shall activate normally in these range
Operating temperature range | -30°C ~ +80°C | Shall conserve normally in these range.
Storage temperature range | -40°C ~ +85°C
Max humidity in use | 95% |
High voltage resistance | 24V/1min, 18V/1hour | After overvoltage is the Normal behavior
Insulation resistance | 100MΩ or more (measured with 500V MEGGER) | Specify as well as parts that insulation like PCB, moisture-proof COATING is required.
Quiescent current | KEYLESS spec : 6mA or less SMK spec : 5mA or less NON-KEYLESS : 3mA or less | Measure when the state, all output loads are OFF and there are no Input SW(including TX operation) changes, continues 2sec.
Voltage drop | 1.2V or less | but, Terminal C01, C02, C03, C13, C14, C16, C19, C21 is 2.0V or less.
Rated Load
No | Item | Rated Road
1 | Room lamp | 30W
2 | KEY SOL | MAX 1A (B+)
3 | Front left turn signal lamp | 33W
4 | Front right turn signal lamp | 33W
5 | Front left turn signal lamp | 28W
6 | Front left turn signal lamp | 28W
7 | Rear right seat warmer relay | 200mA
8 | Rear left seat warmer relay | 200mA
9 | Key hole illumination lamp | 1.4W (BULB)
10 | Front wiper relay | 200mA
11 | Flasher sound relay | 200mA
12 | Rear fog lamp relay | 200mA
13 | Assist seat belt indicator | 1.4W (LED)
14 | RPAS off indicator | 1.4W (LED)
15 | Security IND LED | 1.4W (LED)
16 | Auto light sensor power | MAX 1mA