| TUCSON(LM) >2010 > G 2.4 DOHC > Restraint > Seat Belt Pretensioner > Seat Belt Pretensioner (BPT)>Repair procedures |

Removal
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the lower anchor bolt.
3. | Remove the following parts. (Refer to the Body group- Interior trim)
A. | Door scuff trim
B. | Center pillar trim
4. | Remove the upper anchor bolt.
5. | Disconnect the Seat Belt Pretensioner connector.
6. | Loosen the Seat Belt Pretensioner mounting bolt and remove the Seat Belt Pretensioner.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable and wait for at least three minutes.
3. | Install the Seat Belt Pretensioner (BPT) with a bolt.
Tightening torque Bolt B: 39.2 ~ 53.9 Nm (4.0 ~ 5.5 kgf.m, 28.9 ~39.8 lb.ft)
4. | Connect the Seat Belt Pretensioner (BPT) connector.
5. | Install the upper anchor bolts.
Tightening torque : 39.2 ~ 53.9 Nm (4.0 ~ 5.5 kgf.m, 28.9 ~39.8 lb.ft)
6. | Install the following parts. . (Refer to the Body group- Interior trim)
A. | Center pillar trim
B. | Door scuff trim
7. | Install the lower anchor bolts.
Tightening torque : 39.2 ~ 53.9 Nm (4.0 ~ 5.5 kgf.m, 28.9 ~39.8 lb.ft)
8. | Reconnect the battery negative cable.
9. | After installing the Seat Belt Pretensioner (BPT), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.