| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Smart key System>Specifications |

Specifications
Smart Key Unit
Items | Specification
Rated voltage | DC 12V
Operating voltage | DC 9 ~ 16V
Operating temperature | -22°F ~ 167°F (-30°C ~ 75°C)
Load | Max. 2mA
RF Receiver
Items | Specification
Frequency | 315 Mhz
Antenna type | FSK (Frequency Shift Keying)
Smart Key Fob
Items | Specification
Battery | Lithium battery 3V
Distance | 30m
Battery life | More than 2 years
An inappropriately disposed battery can be harmful to the environment and human health. Dispose the battery according to your local law(s) or regulation.
Push buttons | 4 (Door lock / unlock, Tailgate, Panic)
Frequency(Rx) | 125 kHz
Frequency(Tx) | 315 MHz
Numbers | 2EA
Antenna
Items | Specification
Rated voltage | DC 12V
Operating voltage | DC 9 ~ 16V
Operating temperature | -22°F ~ 167°F (-30°C ~ 75°C)
Frequency | 125kHz
Numbers | Interior(3EA), Door(2EA), Bumper(1EA)