| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Audio > Audio Unit>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the hazard lamp switch assembly (A).
Take care not to damage and scratch the hazard lamp switch assembly and its related parts. Apply the protective tapes to the hazard lamp switch assembly and its related parts.
3. | Disconnect the connectors (A).
4. | Remove the center fascia panel (A).
5. | Remove the audio assembly (A) after loosening the mounting screws.
6. | Disconnect the audio connectors and cable (A), then remove the audio unit completely.
When the compact disc is not ejected, do not remove it forcibly.
Installation
1. | Connect the audio unit connectors and cable.
2. | Install the audio unit.
3. | Install the center facia panel.
4. | Install the hazard switch module.
5. | Connect the negative (-) battery terminal.
Make sure the connector are connected in properly. Check the audio system.
Disassembly
1. | When separate the CD rom drive, if necessary, remove the brackets (A) after loosening the screws (6EA).
2. | Remove the screws (4EA) on the head unit and, and then disassemble the top cover (A).
3. | After loosening the screws, remove the CD rom drive (A).
Take care not to damage the cable connectors (B) when removing drive.